**Tech Specs Once And For All**

Staging:
Musician stage: 1200x1200x600 minimum platform on stage right side at
rear audience seating. Company can provide.
Rostrum. Company can provide.
One low rostra, minimum 1200 wide 600 deep. Company can provide.

Lighting:
General stage wash
Specials:
Spot to musician stage in audience
Spot on rostrum, down right
Spot on coffin, centre stage
A disco effect within audience area, preferably mirror ball. Company
can provide.

Sound:
Mic and DI from the musician stage at rear of audience - prefer
speaker to be located nearby. Company can provide