**Tech Specs Once And For All**

Staging:  
Musician stage: 1200x1200x600 minimum platform on stage right side at  
rear audience seating. Company can provide.  
Rostrum. Company can provide.  
One low rostra, minimum 1200 wide 600 deep. Company can provide.  
  
Lighting:  
General stage wash  
Specials:  
Spot to musician stage in audience  
Spot on rostrum, down right  
Spot on coffin, centre stage  
A disco effect within audience area, preferably mirror ball. Company  
can provide.  
  
Sound:  
Mic and DI from the musician stage at rear of audience - prefer  
speaker to be located nearby. Company can provide